**Bid Clarification (Science Lab Thethe High)**

1. Double door fire door should be a Class 1 Fire Door
2. Storeroom to be fitted with a standard burglar gate
3. Contractor to make allowance for siting of existing water lines
4. To supply and fit an Air Conditioner in the room (18 000 BTU)
5. Specification of the Gas pipe: SABS approved gas pipes
6. Specification for water pipe: Copper
7. Side Cabinet Specifications using similar material: 6.5m (L) x 0.8 (H) x2
8. Projector Specifications:

*The supplier shall provide a one (1) projector, with one (1) wall mounted screen, and the projector shall adhere to the following specifications:*

1. *Lumens: 3000*
2. *Resolution: minimum 1920x1080 pixels*
3. *Contrast ratio: minimum 1000:1*
4. *Zoom ratio: minimum 1.5*
5. *Interface: at least HDMI, USB and RS232*
6. Projector Screen

*HD projector screen with REMOTE for opening and closing which will accommodate the computer, video, slide, and overhead projection in the classroom.*

*- 65 Round Housing Case*

*- Matt White Fabric*

*- Fabric Thickness: 0.4mm*

*- Electronic Motor – 220 – 240 V AC*

*- Wired Remote for Control*

*- Black Framed and Black-Backed Screen.*

*- Screen size: 2366\*1429mm*

A white board with a black strip

Description automatically generated